Logo

Description automatically generated

Fluid Power industry standard color coding for hydraulic circuits.

Red - Pressure lines

Blue - Low pressure, generally return lines

Yellow - Metered line where you are slowing down the oil from the normal flow

Green - Inlet lines

Orange - Reduced pressure when you might have used a pressure-reducing valve

Violet - Intensified pressure

White - No pressure at all

Questions? Contact Ernie Parker at [ErnieParker1@msn.com](mailto:ErnieParker1@msn.com).